Section below to be added into F&A with respect to Unexploded Ordnance

Please pass to the respect chair for comment / approval.

**Existing Services & Underground Assets (Including Unexploded Ordnance)** Prior diversion or removal of services/assets to facilitate installation of the Specialist Works and, where required by the owner of the service/asset, written evidence confirming no services/assets are present and/or that work may proceed. Exposing on site or accurate, clear and robust marking of the exact location of remaining overhead or underground services/assets and providing a drawing on which their positions in line and level are accurately plotted relative to the Specialist Works. The location and sealing off of all live or disused pipes, ducts or the like to prevent the entry of concrete, grout, slurry or drilling fluids etc. during construction. Subsequent to the foregoing the Specialist’s authorised representative is to be issued with a Permit to Dig or similar authorisation on a daily basis or as otherwise agreed.

**Unexploded Ordnance –** Prior risk assessment, risk mitigation, management implementation and emergency response plans to be in place where a risk from UXO is identified.